<config configName="default" projectName="Pstat_AD5941_11apr22" configVersion="1.1" device="PIC24F16KM202" deviceLibraryClass="com.microchip.mcc.mcu16.Mcu16PeripheralLibrary" coreVersion="5.4.11">
   <usedPackages class="java.util.ArrayList"/>
   <usedClasses class="java.util.TreeMap">
      <entry>
         <string>ADC1</string>
         <string>class com.microchip.mcc.mcu16.modules.adc.ADC</string>
      </entry>
      <entry>
         <string>DELAY</string>
         <string>class com.microchip.mcc.foundationservices.modules.softwaredriver.delay.DELAY</string>
      </entry>
      <entry>
         <string>ICD</string>
         <string>class com.microchip.mcc.mcu16.systemManager.icd.Icd</string>
      </entry>
      <entry>
         <string>INTERNAL OSCILLATOR</string>
         <string>class com.microchip.mcc.mcu16.systemManager.clk.Clock</string>
      </entry>
      <entry>
         <string>Interrupt Module</string>
         <string>class com.microchip.mcc.mcu16.interruptManager.InterruptManager</string>
      </entry>
      <entry>
         <string>Main Manager</string>
         <string>class com.microchip.mcc.mcu16.mainManager.MainManager</string>
      </entry>
      <entry>
         <string>Pin Module</string>
         <string>class com.microchip.mcc.mcu16.pinManager.PinManager</string>
      </entry>
      <entry>
         <string>RESET</string>
         <string>class com.microchip.mcc.mcu16.systemManager.reset.RESET</string>
      </entry>
      <entry>
         <string>System Module</string>
         <string>class com.microchip.mcc.mcu16.systemManager.DefaultSystemManagerMcu16</string>
      </entry>
      <entry>
         <string>UART2</string>
         <string>class com.microchip.mcc.mcu16.modules.uart.UART</string>
      </entry>
      <entry>
         <string>WATCHDOG</string>
         <string>class com.microchip.mcc.mcu16.systemManager.wdt.Wdt</string>
      </entry>
      <entry>
         <string>com.microchip.mcc.boardsupportlibrary.BoardSuppportLibraryLibraryModule</string>
         <string>class com.microchip.mcc.protocolServices.base.modules.librarymodule.LibraryModule</string>
      </entry>
      <entry>
         <string>com.microchip.mcc.mcu16.Mcu16PeripheralLibraryLibraryModule</string>
         <string>class com.microchip.mcc.protocolServices.base.modules.librarymodule.LibraryModule</string>
      </entry>
   </usedClasses>
   <usedLibraries class="java.util.ArrayList">
      <ILibraryFile class="com.microchip.mcc.core.library.BaseLibraryFile" libraryClass="com.microchip.mcc.mcu16.Mcu16PeripheralLibrary" version="1.171.1"/>
      <ILibraryFile class="com.microchip.mcc.core.library.BaseLibraryFile" libraryClass="com.microchip.mcc.foundationservices.library.FoundationServicesLibrary" version="0.2.3"/>
      <ILibraryFile class="com.microchip.mcc.core.library.BaseLibraryFile" libraryClass="com.microchip.mcc.boardsupportlibrary.BoardSuppportLibrary" version="1.12.0"/>
   </usedLibraries>
   <tokenMap class="java.util.TreeMap">
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="ADC1_ADIISRFunction"/>
         <value>ISR_ADC1_ADI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="ADCFunctionMode"/>
         <value>ADC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN13"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN15"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN16"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN17"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN18"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN19"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN20"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN21"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN4"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN5"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AN9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AVDD"/>
         <value>CHANNEL_AVDD</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="AVSS"/>
         <value>CHANNEL_AVSS</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="CTMU"/>
         <value>CHANNEL_CTMU</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="CTMU temperature sensor input"/>
         <value>CHANNEL_CTMU temperature sensor input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="Internal Band Gap Reference"/>
         <value>CHANNEL_Internal Band Gap Reference</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="Lower guardband rail"/>
         <value>CHANNEL_Lower guardband rail</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="SCAN_ENABLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="Scan_Count"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="Upper guardband rail"/>
         <value>CHANNEL_Upper guardband rail</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="adcsCustomKey"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="localClockKey"/>
         <value>4000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ADC1" name="tad"/>
         <value>0.000016000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH16" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH16" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH17" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH17" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH18" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH18" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH19" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH19" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH20" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH20" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH21" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH21" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH22" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH22" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH23" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH23" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NA" alias="AN0"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NA" alias="AN1"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NA" alias="AN2"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NA" alias="AN3"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NA" alias="AN4"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NA" alias="AN5"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NA" alias="AVSS"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NB" alias="AN0"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NB" alias="AN1"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NB" alias="AN2"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NB" alias="AN3"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NB" alias="AN4"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NB" alias="AN5"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NB" alias="AVSS"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN10"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN11"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN12"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN13"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN14"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN15"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN16"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN17"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN18"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN19"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN20"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN21"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN4"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN5"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AN9"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AVDD"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="AVSS"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="CTMU"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="CTMU temperature sensor input"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="Internal Band Gap Reference"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="Lower guardband rail"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA" alias="Upper guardband rail"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN10"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN11"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN12"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN13"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN14"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN15"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN16"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN17"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN18"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN19"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN20"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN21"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN4"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN5"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AN9"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AVDD"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="AVSS"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="CTMU"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="CTMU temperature sensor input"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="Internal Band Gap Reference"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="Lower guardband rail"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB" alias="Upper guardband rail"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ADON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ADON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ADSIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ADSIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ASAM" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ASAM" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="DONE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="DONE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="FORM" alias="Absolute decimal result, unsigned, right-justified"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="FORM" alias="Absolute fractional result, unsigned, left-justified"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="FORM" alias="Decimal result, signed, right-justified"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="FORM" alias="Fractional result, signed, left-justified"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="MODE12" alias="10-bit"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="MODE12" alias="12-bit"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SAMP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SAMP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="CLC1"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="CLC2"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="CTMU"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="Clearing sample bit ends sampling and starts conversion"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="INT0"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="Internal counter ends sampling and starts conversion"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="MCCP1"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="MCCP2"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="MCCP3"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="SCCP4"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="SCCP5"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="TMR1"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC" alias="TMR1 Sleep"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="ALTS" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="ALTS" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFM" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFM" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFREGEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFREGEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFS" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFS" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="CSCNA" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="CSCNA" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="NVCFG0" alias="AVSS"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="NVCFG0" alias="VREF-"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="OFFCAL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="OFFCAL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="PVCFG" alias="2 * Internal VBG"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="PVCFG" alias="AVDD"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="PVCFG" alias="VREF+"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 10th sample/conversion operation"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 11th sample/conversion operation"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 12th sample/conversion operation"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 13th sample/conversion operation"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 14th sample/conversion operation"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 15th sample/conversion operation"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 16th sample/conversion operation"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 17th sample/conversion operation"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 18th sample/conversion operation"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 19th sample/conversion operation"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 20th sample/conversion operation"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 21th sample/conversion operation"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 22nd sample/conversion operation"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 23rd sample/conversion operation"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 24th sample/conversion operation"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 25th sample/conversion operation"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 26th sample/conversion operation"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 27th sample/conversion operation"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 28th sample/conversion operation"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 29th sample/conversion operation"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 2nd sample/conversion operation"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 30th sample/conversion operation"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 31th sample/conversion operation"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 32nd sample/conversion operation"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 3rd sample/conversion operation"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 4th sample/conversion operation"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 5th sample/conversion operation"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 6th sample/conversion operation"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 7th sample/conversion operation"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 8th sample/conversion operation"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every 9th sample/conversion operation"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI" alias="Generates interrupt after completion of every sample/conversion operation"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="ADRC" alias="FOSC/2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="ADRC" alias="RC clock"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="EXTSAM" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="EXTSAM" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="10"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="11"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="12"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="13"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="14"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="15"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="16"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="17"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="18"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="19"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="20"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="21"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="22"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="23"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="24"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="25"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="26"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="27"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="28"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="29"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="30"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="31"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="4"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="5"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="6"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="7"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="8"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC" alias="9"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="ASEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="ASEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="ASINT" alias="Interrupt after Threshold Detect sequence is completed"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="ASINT" alias="Interrupt after Threshold Detect sequence is completed and a valid compare has occurred"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="ASINT" alias="Interrupt after valid compare has occurred"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="ASINT" alias="No interrupt"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="BGREQ" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="BGREQ" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="CM" alias="Greater Than mode"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="CM" alias="Inside Window mode"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="CM" alias="Less Than mode"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="CM" alias="Outside Window mode"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="CTMREQ" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="CTMREQ" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="LPEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="LPEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="WM" alias="Auto-compare only"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="WM" alias="Convert and save"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="WM" alias="Legacy operation"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS16" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS16" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS17" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS17" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS18" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS18" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS19" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS19" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS20" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS20" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS21" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS21" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS22" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS22" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS23" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS23" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS26" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS26" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS27" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS27" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS28" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS28" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS29" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS29" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS30" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS30" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN16" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN16" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN17" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN17" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN18" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN18" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN19" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN19" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN20" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN20" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN21" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN21" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN22" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN22" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN23" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN23" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCHITH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCHITL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCHS"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCON1"/>
         <value>33904</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCON2"/>
         <value>32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCON3"/>
         <value>7999</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCON5"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCSSH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCSSL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCTMENH"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="ADC1" registerAlias="ADCTMENL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH16"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH17"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH18"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH19"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH20"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH21"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH22"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITH" settingAlias="CHH23"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHITL" settingAlias="CHH9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NA"/>
         <value>AVSS</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0NB"/>
         <value>AVSS</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SA"/>
         <value>AN0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCHS" settingAlias="CH0SB"/>
         <value>AN0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ADON"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ADSIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="ASAM"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="DONE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="FORM"/>
         <value>Absolute decimal result, unsigned, right-justified</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="MODE12"/>
         <value>12-bit</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SAMP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON1" settingAlias="SSRC"/>
         <value>Internal counter ends sampling and starts conversion</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="ALTS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFM"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFREGEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="BUFS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="CSCNA"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="NVCFG0"/>
         <value>AVSS</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="OFFCAL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="PVCFG"/>
         <value>2 * Internal VBG</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON2" settingAlias="SMPI"/>
         <value>Generates interrupt after completion of every sample/conversion operation</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="ADCS"/>
         <value>63</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="ADRC"/>
         <value>FOSC/2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="EXTSAM"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON3" settingAlias="SAMC"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="ASEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="ASINT"/>
         <value>No interrupt</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="BGREQ"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="CM"/>
         <value>Less Than mode</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="CTMREQ"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="LPEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCON5" settingAlias="WM"/>
         <value>Legacy operation</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS16"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS17"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS18"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS19"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS20"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS21"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS22"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS23"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS26"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS27"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS28"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS29"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSH" settingAlias="CSS30"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCSSL" settingAlias="CSS9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN16"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN17"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN18"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN19"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN20"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN21"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN22"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENH" settingAlias="CTMEN23"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADCTMENL" settingAlias="CTMEN9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="ADC1" registerAlias="ADI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="DELAY" name="usecaseComboSettings"/>
         <value>None</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ICD" name="customICS"/>
         <value>EMUC/EMUD share PGC2/PGD2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ICD" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLKPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLKPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FOSC"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FOSC2"/>
         <value>4000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FRC"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_LPRC"/>
         <value>31000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_PRIMARY"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_SOSC"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_USB"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="ClockSource"/>
         <value>FRC Oscillator</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="ClockSwitching"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FailSafe"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAutoTune"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockChange"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockFBDivisor"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPostscaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPostscaler2"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPrescaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockSource"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxPll"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAvcoDivider"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureCANFDClock"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockChange"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockSource"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockSwitching"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureCodeGuard"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureFrcEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureFrcScaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureIESOUpdate"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureOscfDivisor"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureOscfdivEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllCpuDivScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllDisplayScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllEnable"/>
         <value>NOTAVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllFeedbackDivisor"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllGraphicsSelect"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllPostScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllTwoStagePostScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePoscErrataWorkaround"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefClkOutoutEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockDivSwitch"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockDivider"/>
         <value>NOTAVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockSource"/>
         <value>NOTAVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockTrim"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoOutputPinEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureSoscClock"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureSoscEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureUsb"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureVcoDivider"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcEnable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcPostscaler"/>
         <value>1:2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcPostscalerClock"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="OSCPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="OSCPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllClock"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllEnable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="Pll_Dependent_Clock_Switching"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_ENABLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_INPUT_FREQUENCY"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_RODIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_ROSEL"/>
         <value>FOSC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFOPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFOPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="Requested CAN Clock Frequency"/>
         <value>20000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SCLKPinsInput"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SOSCPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SOSCPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UI_OSCTUN_SETTING"/>
         <value>Center frequency</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UseSosc"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="customClkOut"/>
         <value>Port I/O enabled (CLKO disabled)</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:128"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/256"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="ROI" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="ROI" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF" alias="clock failure"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF" alias="no clock failure"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK" alias="locked"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK" alias="unlocked"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRCDIV"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRCPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="LPFRC"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="PRIPLL"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="SOSC"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="LOCK" alias="in lock"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="LOCK" alias="out of lock"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRCDIV"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRCPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="LPFRC"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="PRIPLL"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="SOSC"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN" alias="Request Switch"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN" alias="Switch is Complete"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SOSCDRV" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SOSCDRV" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SOSCEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SOSCEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.164%"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.328%"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.492%"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.656%"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.820%"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.984%"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.148%"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.312%"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.476%"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.640%"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.804%"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.968%"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+2.132%"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+2.296%"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+2.460%"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+2.624%"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+2.788%"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+2.952%"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+3.116%"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+3.280%"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+3.444%"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+3.608%"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+3.772%"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+3.936%"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+4.100%"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+4.264%"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+4.428%"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+4.592%"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+4.756%"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+4.920%"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.164%"/>
         <value>63</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.328%"/>
         <value>62</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.492%"/>
         <value>61</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.656%"/>
         <value>60</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.820%"/>
         <value>59</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.984%"/>
         <value>58</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.148%"/>
         <value>57</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.312%"/>
         <value>56</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.476%"/>
         <value>55</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.640%"/>
         <value>54</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.804%"/>
         <value>53</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.968%"/>
         <value>52</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-2.132%"/>
         <value>51</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-2.296%"/>
         <value>50</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-2.460%"/>
         <value>49</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-2.624%"/>
         <value>48</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-2.788%"/>
         <value>47</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-2.952%"/>
         <value>46</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-3.116%"/>
         <value>45</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-3.280%"/>
         <value>44</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-3.444%"/>
         <value>43</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-3.608%"/>
         <value>42</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-3.772%"/>
         <value>41</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-3.936%"/>
         <value>40</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-4.100%"/>
         <value>39</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-4.264%"/>
         <value>38</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-4.428%"/>
         <value>37</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-4.592%"/>
         <value>36</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-4.756%"/>
         <value>35</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-4.920%"/>
         <value>34</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-5.084%"/>
         <value>33</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center frequency"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Maximum frequency deviation"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Minimum frequency deviation"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="ADC1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="ADC1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SSP1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SSP1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP3MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP3MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP4MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP4MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP5MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP5MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CMPMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CMPMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="DAC1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="DAC1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="RTCCMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="RTCCMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="SSP2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="SSP2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="CTMUMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="CTMUMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="HLVDMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="HLVDMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="REFOMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="REFOMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="ULPWUMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="ULPWUMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="AMP1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="AMP1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="AMP2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="AMP2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DAC2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DAC2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL" alias="FOSC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL" alias="Primary Oscillator"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSSLP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSSLP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV"/>
         <value>12544</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE"/>
         <value>1:8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV"/>
         <value>FRC/2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="ROI"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF"/>
         <value>no clock failure</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK"/>
         <value>unlocked</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC"/>
         <value>FRCDIV</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="LOCK"/>
         <value>out of lock</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC"/>
         <value>FRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN"/>
         <value>Switch is Complete</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SOSCDRV"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SOSCEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN"/>
         <value>Center frequency</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="ADC1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SSP1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP4MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="CCP5MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CMPMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="DAC1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="RTCCMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="SSP2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="CTMUMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="HLVDMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="REFOMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD4" settingAlias="ULPWUMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="AMP1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="AMP2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD6" settingAlias="DAC2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD8" settingAlias="CLC2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="RODIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL"/>
         <value>FOSC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSSLP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA2"/>
         <value>channel_AN13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA4"/>
         <value>channel_AN16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA5"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA6"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA7"/>
         <value>IO_RA7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB10"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB11"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB12"/>
         <value>IO_RB12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB13"/>
         <value>IO_RB13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB14"/>
         <value>IO_RB14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB15"/>
         <value>IO_RB15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB2"/>
         <value>channel_AN4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB3"/>
         <value>channel_AN5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB4"/>
         <value>channel_AN15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB5"/>
         <value>IO_RB5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB6"/>
         <value>IO_RB6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB7"/>
         <value>channel_AN19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB8"/>
         <value>IO_RB8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB9"/>
         <value>channel_AN21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Pin Module_CNIISRFunction"/>
         <value>ISR_Pin Module_CNI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB12"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB13"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB14"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB15"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB5"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB6"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB8"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA3"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB10"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB11"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB12"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB13"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB14"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB15"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB8"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB9"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="packageId"/>
         <value>PDIP28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA3"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA0" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA0" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA1" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA1" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA2" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA2" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA3" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA3" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA4" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA4" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB0" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB0" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB1" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB1" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB12" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB12" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB13" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB13" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB14" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB14" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB15" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB15" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB2" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB2" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB3" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB3" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB4" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB4" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB5" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB5" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB6" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB6" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB7" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB7" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB8" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB8" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB9" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB9" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN0IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN0IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN11IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN11IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN12IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN12IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN13IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN13IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN14IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN14IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN15IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN15IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN1IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN1IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN2IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN2IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN3IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN3IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN4IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN4IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN5IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN5IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN6IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN6IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN7IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN7IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN8IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN8IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN9IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN9IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN16IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN16IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN21IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN21IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN22IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN22IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN23IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN23IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN24IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN24IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN27IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN27IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN29IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN29IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN30IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN30IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN0PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN0PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN11PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN11PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN12PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN12PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN13PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN13PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN14PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN14PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN15PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN15PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN1PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN1PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN2PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN2PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN3PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN3PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN4PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN4PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN5PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN5PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN6PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN6PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN7PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN7PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN8PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN8PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN9PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN9PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN16PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN16PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN21PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN21PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN22PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN22PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN23PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN23PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN24PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN24PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN27PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN27PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN29PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN29PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN30PDE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN30PDE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN0PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN0PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN11PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN11PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN12PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN12PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN13PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN13PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN14PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN14PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN15PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN15PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN1PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN1PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN2PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN2PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN3PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN3PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN4PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN4PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN5PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN5PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN6PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN6PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN7PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN7PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN8PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN8PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN9PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN9PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN16PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN16PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN21PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN21PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN22PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN22PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN23PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN23PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN24PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN24PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN27PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN27PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN29PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN29PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN30PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN30PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB12" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB12" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCONA" settingAlias="ODA5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCONA" settingAlias="ODA5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA5" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA5" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB12" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB12" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ANSA"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ANSB"/>
         <value>668</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPD1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPD2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPU1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPU2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATB"/>
         <value>8193</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCONA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISA"/>
         <value>247</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISB"/>
         <value>3742</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA0"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA1"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA2"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA3"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSA" settingAlias="ANSELA4"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB0"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB1"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB12"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB13"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB14"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB15"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB2"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB3"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB4"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB5"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB6"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB7"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB8"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSB" settingAlias="ANSELB9"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN0IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN11IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN12IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN13IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN14IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN15IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN1IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN2IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN3IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN4IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN5IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN6IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN7IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN8IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN9IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN16IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN21IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN22IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN23IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN24IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN27IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN29IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN30IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN0PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN11PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN12PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN13PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN14PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN15PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN1PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN2PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN3PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN4PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN5PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN6PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN7PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN8PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD1" settingAlias="CN9PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN16PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN21PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN22PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN23PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN24PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN27PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN29PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPD2" settingAlias="CN30PDE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN0PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN11PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN12PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN13PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN14PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN15PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN1PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN2PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN3PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN4PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN5PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN6PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN7PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN8PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN9PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN16PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN21PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN22PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN23PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN24PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN27PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN29PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN30PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0"/>
         <value>set</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB12"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13"/>
         <value>set</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCONA" settingAlias="ODA5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA5"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA6"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB12"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="BOR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="BOR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="CM" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="CM" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="EXTR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="EXTR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IDLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IDLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IOPUWR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IOPUWR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="PMSLP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="PMSLP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="POR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="POR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SLEEP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SLEEP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWDTEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWDTEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="TRAPR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="TRAPR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="WDTO" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="WDTO" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="RESET" registerAlias="RCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="BOR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="CM"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="EXTR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="IDLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="IOPUWR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="PMSLP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="POR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="SLEEP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWDTEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="TRAPR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="WDTO"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FBS" settingAlias="BSS" alias="HI1K"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FBS" settingAlias="BSS" alias="HI2K"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FBS" settingAlias="BSS" alias="OFF"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FBS" settingAlias="BSS" alias="STD1K"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FBS" settingAlias="BSS" alias="STD2K"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FBS" settingAlias="BWRP" alias="OFF"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FBS" settingAlias="BWRP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FGS" settingAlias="GCP" alias="OFF"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FGS" settingAlias="GCP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FGS" settingAlias="GWRP" alias="OFF"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FGS" settingAlias="GWRP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="PGx1"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="PGx2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="PGx3"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="FCKSM" alias="CSDCMD"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="FCKSM" alias="CSECMD"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="FCKSM" alias="CSECME"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="OSCIOFCN" alias="OFF"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="OSCIOFCN" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCFREQ" alias="HS"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCFREQ" alias="LS"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCFREQ" alias="MS"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD" alias="EC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD" alias="HS"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD" alias="NONE"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD" alias="XT"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="SOSCSEL" alias="SOSCHP"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSC" settingAlias="SOSCSEL" alias="SOSCLP"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="FRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="FRCDIV"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="FRCPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="LPFRC"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="PRIPLL"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="SOSC"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="IESO" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="IESO" alias="ON"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="LPRCSEL" alias="HP"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="LPRCSEL" alias="LP"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="SOSCSRC" alias="ANA"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="SOSCSRC" alias="DIG"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN" alias="BOR0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN" alias="BOR1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN" alias="BOR2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN" alias="BOR3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BORV" alias="LPBOR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BORV" alias="V18"/>
         <value>96</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BORV" alias="V27"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BORV" alias="V30"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="I2C1SEL" alias="PRI"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="I2C1SEL" alias="SEC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="MCLRE" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="MCLRE" alias="ON"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="PWRTEN" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="PWRTEN" alias="ON"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN" alias="NOSLP"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN" alias="ON"/>
         <value>160</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN" alias="SWON"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWPSA" alias="PR128"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWPSA" alias="PR32"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS1024"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS128"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS16384"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS2048"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS256"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS32768"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS4096"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS512"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS8192"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WINDIS" alias="OFF"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WINDIS" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FBS"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FGS"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FICD"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FOSC"/>
         <value>187</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FOSCSEL"/>
         <value>96</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FPOR"/>
         <value>251</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FWDT"/>
         <value>222</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FBS" settingAlias="BSS"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FBS" settingAlias="BWRP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FGS" settingAlias="GCP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FGS" settingAlias="GWRP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS"/>
         <value>PGx2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="FCKSM"/>
         <value>CSDCMD</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="OSCIOFCN"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCFREQ"/>
         <value>HS</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="POSCMOD"/>
         <value>NONE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSC" settingAlias="SOSCSEL"/>
         <value>SOSCHP</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC"/>
         <value>FRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="IESO"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="LPRCSEL"/>
         <value>HP</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="SOSCSRC"/>
         <value>ANA</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN"/>
         <value>BOR3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BORV"/>
         <value>V18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FPOR" settingAlias="I2C1SEL"/>
         <value>PRI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FPOR" settingAlias="MCLRE"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FPOR" settingAlias="PWRTEN"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN"/>
         <value>SWON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWPSA"/>
         <value>PR128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS"/>
         <value>PS16384</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WINDIS"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="AllInterrupts"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="BaudRate"/>
         <value>9600</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="BaudRateError"/>
         <value>0.160</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="DataBits"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="FlowControl"/>
         <value>None</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="InternalClock"/>
         <value>4000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="Parity"/>
         <value>None</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="RedirectPrintf"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="SWRXBufferSize"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="SWTXBufferSize"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="UART2_UERIISRFunction"/>
         <value>ISR_UART2_UERI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="UART2_URXIISRFunction"/>
         <value>ISR_UART2_URXI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="UART2_UTXIISRFunction"/>
         <value>ISR_UART2_UTXI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="UARTFunctionMode"/>
         <value>UART</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="UCTS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="URTS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="URX"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="UTX"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="inputmode"/>
         <value>easysetup</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="ABAUD" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="ABAUD" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="BRGH" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="BRGH" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="IREN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="IREN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="LPBACK" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="LPBACK" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="PDSEL" alias="8E"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="PDSEL" alias="8N"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="PDSEL" alias="8O"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="PDSEL" alias="9N"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="RTSMD" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="RTSMD" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="STSEL" alias="1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="STSEL" alias="2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UARTEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UARTEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UEN" alias="TX_RX"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UEN" alias="TX_RX_BCLK"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UEN" alias="TX_RX_CTS_RTS"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="URXINV" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="URXINV" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="USIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="USIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="WAKE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="WAKE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="ADDEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="ADDEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="FERR" alias="ERROR"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="FERR" alias="NO_ERROR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="OERR" alias="ERROR"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="OERR" alias="NO_ERROR_cleared"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="PERR" alias="ERROR"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="PERR" alias="NO_ERROR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="RIDLE" alias="ACTIVE"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="RIDLE" alias="IDLE"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="TRMT" alias="EMPTY"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="TRMT" alias="NOT_EMPTY"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXDA" alias="EMPTY"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXDA" alias="HAS_DATA"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXISEL" alias="RX_3_4_BUF_FULL"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXISEL" alias="RX_BUF_FULL"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXISEL" alias="RX_ONE_CHAR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXBF" alias="FULL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXBF" alias="NOT_FULL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXBRK" alias="COMPLETED"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXBRK" alias="SEND"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXINV" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXINV" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXISEL" alias="TX_BUF_EMPTY"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXISEL" alias="TX_COMPLETE"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXISEL" alias="TX_ONE_CHAR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="UART2" registerAlias="UBRG"/>
         <value>103</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="UART2" registerAlias="UMODE"/>
         <value>32776</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="UART2" registerAlias="USTA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="UART2" registerAlias="UTXREG"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UBRG" settingAlias="BRG"/>
         <value>103</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UERI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UERI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UERI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UERI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="ABAUD"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="BRGH"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="IREN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="LPBACK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="PDSEL"/>
         <value>8N</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="RTSMD"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="STSEL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UARTEN"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UEN"/>
         <value>TX_RX</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="URXINV"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="USIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="WAKE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="URXI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="URXI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="URXI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="URXI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="ADDEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="FERR"/>
         <value>NO_ERROR</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="OERR"/>
         <value>NO_ERROR_cleared</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="PERR"/>
         <value>NO_ERROR</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="RIDLE"/>
         <value>IDLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="TRMT"/>
         <value>EMPTY</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXDA"/>
         <value>EMPTY</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXISEL"/>
         <value>RX_ONE_CHAR</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXBF"/>
         <value>NOT_FULL</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXBRK"/>
         <value>COMPLETED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXINV"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXISEL"/>
         <value>TX_ONE_CHAR</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UTXI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UTXI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UTXI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UTXI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UTXREG" settingAlias="UTXREG"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="ClockInput"/>
         <value>31000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="TimerPeriod"/>
         <value>67.650s</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="clockSourceSelect"/>
         <value>CLOCK_LPRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="customFWDTEN"/>
         <value>WDT controlled with the SWDTEN bit setting</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="customViewerUpdate"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="customWDTPS"/>
         <value>1:16384</value>
      </entry>
   </tokenMap>
   <generatedFileHashHistoryMap class="java.util.TreeMap">
      <entry>
         <file>main.c</file>
         <hash>380c2097cf729647fe548615e574ca40fd007a6634618d65d317793ad306d471</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\adc1.c</file>
         <hash>f4c36b889595fb32c78b7f3a0177dc141e0017b080af89533ad133eb22b1aad5</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\adc1.h</file>
         <hash>13838c053419ac52c5e55e6dec845b68937cecfd919c6470e3f11a77ca664cab</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\adc_module_features.h</file>
         <hash>a6950289abfb0a34686dd1b5e4c0464465e67dadcea806bff05fc09c6110c1e7</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\clock.c</file>
         <hash>6da7af5780ff92ef221eae5c8db4b67f65828bae4193672278542d5e41139ec7</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\clock.h</file>
         <hash>b41435580c0ab019edeaff444c8a24ecfb6b17fbd4371b5b10852c559de9b0ff</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\delay.c</file>
         <hash>4a6b8bbd5d2fbe5f20e79db8d915e50e2cd43920940679b40db90f3789cbccd5</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\delay.h</file>
         <hash>dda77102dba9adc0f9aef1c8c542cfee6d6cccc96446f4cd1bf07be2150a4d95</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\docs\delay.dox</file>
         <hash>13d4874d789b563dd4499efacd71882cbc38f8459da91ac17f13fa76079be93b</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\interrupt_manager.c</file>
         <hash>7b3218a3e3ece234ffe395bdb1dd1adc4c655ecd96426c2db1baee8f92581f23</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\interrupt_manager.h</file>
         <hash>a5db4c34c49e0fa7d496303f5d51c5e785fb73a247e31141350fec4b174d4584</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\mcc.c</file>
         <hash>b9f55a64f3afff16b955271abf861d1c52e464df0f6ab58e30f2e3b5dfbb7629</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\mcc.h</file>
         <hash>2b36a7280d0a147780b2ab233c46a8eb10dd2f51b09c93476a983517f20ffe5e</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pin_manager.c</file>
         <hash>0669714df817a0503a60f73b5ccf20d7f05d404b39ef763e6ea33b356cca8e10</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pin_manager.h</file>
         <hash>1140142ab668b9f1c915c88ebddcaab7dd5301d5f664b9b1b14741c774da9876</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system.c</file>
         <hash>efe284e0e99e61b09ca3c8c7aac1cb402b02c4eed19033ace06d92872f633a84</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system.h</file>
         <hash>8aaed003ec0e67dab7c4989fee36b15eeb68aa308a5a67bc78b766a176cb76bf</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\traps.c</file>
         <hash>da28ff9277b1928e900927f262b0d052880dcb37d8c27a25923e546963eaf697</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\traps.h</file>
         <hash>6e692bac7565988104286214b43caacb1c041211ced859fc2e1fcefb9344e6a1</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\uart2.c</file>
         <hash>d25b362ef02be57f6bb13fc967e797e1ffbb9fd9e64e61b6736174d44d836c56</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\uart2.h</file>
         <hash>94cedee519bb3f8e38fb21d6d73c73c21126091155559257e22b311794ae8996</hash>
      </entry>
   </generatedFileHashHistoryMap>
</config>